WANPIPE ANALOG TAPPING



* Wed July 16 2008
========================================================================
Enabling Tapping Mode

Linux:
-Add RM_MODE = RM_TAPPING in wanpipeX section of wanpipex.conf

Windows:
-In Device Manager->Sangoma Hardware Abstraction Driver (Analog)->
	Analog Modules->Miscellenious Interface Options->FXO Tapping, set it
	to "On".
	
Notes:

- When line is unplugged, "Disconnect" event follows "Off-hook" event because 
  Off-hook also means no battery on the line. Only handle "Disconnect" event
  in this situation. There is at least 5 seconds delay between these two 
  events.   

- Connect/Disconnect events are only valid for FXO modules
