;/*++
;
;Copyright (c) 1984-2012 Sangoma Technologies All rights Reserved
;
;Module Name:
;    sdladrv.inf
;
;Author:
;	David Rokhvarg <davidr@sangoma.com>
;
;Description:
;    Inf File for installing Sangoma Hardware Abstraction driver on Windows XP/2003/2008/7.
;
;--*/

[Version]
Signature	= "$Windows NT$"
class		= SANGOMA_ADAPTER
classGUID	= {680D0063-63ED-4e66-A2CC-6F54CB331CF5}
Provider	= %V_Sangoma%
DriverVer   = 10/28/2016, 7.0.20.7

CatalogFile.ntx86=sdladrv.ntx86.cat
CatalogFile.NTamd64=sdladrv.ntX64.cat

[DestinationDirs]
DefaultDestDir	    = 12
Drivers_Dir         = 12 ;system32\drivers
system32.CopyFiles  = 11 ;system32

[ClassInstall32.ntx86]
Addreg=SangomaAdapterClassReg     

[ClassInstall32.ntamd64]
Addreg=SangomaAdapterClassReg     

[SangomaAdapterClassReg]
HKR,,,0,%ClassName%

[SourceDisksNames.x86]
1 = %DiskId1%,,,""
2 = %DiskId1%,,,\x86

[SourceDisksNames.amd64]
1 = %DiskId1%,,,""
2 = %DiskId1%,,,\x64

[SourceDisksFiles]
sdladrv.sys			= 2,,
sdlacfg.dll			= 2,,
wan_aftup.exe		= 2,,
wanec_client.exe	= 2,,
stelephony.dll		= 2,,
libsangoma.dll		= 2,,
waneclib.dll		= 2,,
wanpipemon.exe		= 2,,
stail.exe			= 2,,
wan_xilinx_test.exe	= 2,,
wanrouter.exe		= 2,,
wancfglib.dll		= 2,,

;*****************************************
; Install Section
;*****************************************

[Manufacturer]
%V_Sangoma%=Sangoma,NTx86,NTamd64

[Sangoma.NTx86]
;S518-ADSL. Using ADSL section.
%SangomaVirtualAdapter_AFT__ADSL.DeviceDesc%=SangomaVirtualAdapter_ADSL,   CommsAdapter\SangomaAdapter_S518_ADSL
; A101/2/4/8-T1/E1 and A116/T116 and A140-Serial
%SangomaVirtualAdapter_AFT_Line1.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE1
%SangomaVirtualAdapter_AFT_Line2.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE2
%SangomaVirtualAdapter_AFT_Line3.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE3
%SangomaVirtualAdapter_AFT_Line4.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE4
%SangomaVirtualAdapter_AFT_Line5.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE5
%SangomaVirtualAdapter_AFT_Line6.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE6
%SangomaVirtualAdapter_AFT_Line7.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE7
%SangomaVirtualAdapter_AFT_Line8.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE8
%SangomaVirtualAdapter_AFT_Line9.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE9
%SangomaVirtualAdapter_AFT_Line10.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE10
%SangomaVirtualAdapter_AFT_Line11.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE11
%SangomaVirtualAdapter_AFT_Line12.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE12
%SangomaVirtualAdapter_AFT_Line13.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE13
%SangomaVirtualAdapter_AFT_Line14.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE14
%SangomaVirtualAdapter_AFT_Line15.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE15
%SangomaVirtualAdapter_AFT_Line16.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE16
;A200 - analog
%SangomaVirtualAdapter_AFT__A200.DeviceDesc%=SangomaVirtualAdapter_Analog, CommsAdapter\SangomaAdapter_AFT__A200
;AFT-56k
%SangomaVirtualAdapter_AFT_Line1.DeviceDesc%=SangomaVirtualAdapter_56k,    CommsAdapter\SangomaAdapter_A056__56K
;AFT-ISDN BRI
%SangomaVirtualAdapter_AFT__A500.DeviceDesc%=SangomaVirtualAdapter_BRI,    CommsAdapter\SangomaAdapter_A500__BRI

[Sangoma.NTamd64]
;S518-ADSL. Using ADSL section.
%SangomaVirtualAdapter_AFT__ADSL.DeviceDesc%=SangomaVirtualAdapter_ADSL,   CommsAdapter\SangomaAdapter_S518_ADSL
; A101/2/4/8-T1/E1 and A116/T116 and A140-Serial
%SangomaVirtualAdapter_AFT_Line1.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE1
%SangomaVirtualAdapter_AFT_Line2.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE2
%SangomaVirtualAdapter_AFT_Line3.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE3
%SangomaVirtualAdapter_AFT_Line4.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE4
%SangomaVirtualAdapter_AFT_Line5.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE5
%SangomaVirtualAdapter_AFT_Line6.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE6
%SangomaVirtualAdapter_AFT_Line7.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE7
%SangomaVirtualAdapter_AFT_Line8.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE8
%SangomaVirtualAdapter_AFT_Line9.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE9
%SangomaVirtualAdapter_AFT_Line10.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE10
%SangomaVirtualAdapter_AFT_Line11.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE11
%SangomaVirtualAdapter_AFT_Line12.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE12
%SangomaVirtualAdapter_AFT_Line13.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE13
%SangomaVirtualAdapter_AFT_Line14.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE14
%SangomaVirtualAdapter_AFT_Line15.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE15
%SangomaVirtualAdapter_AFT_Line16.DeviceDesc%=SangomaVirtualAdapter, 	   CommsAdapter\SangomaAdapter_AFT_LINE16
;A200 - analog
%SangomaVirtualAdapter_AFT__A200.DeviceDesc%=SangomaVirtualAdapter_Analog, CommsAdapter\SangomaAdapter_AFT__A200
;AFT-56k
%SangomaVirtualAdapter_AFT_Line1.DeviceDesc%=SangomaVirtualAdapter_56k,    CommsAdapter\SangomaAdapter_A056__56K
;AFT-ISDN BRI
%SangomaVirtualAdapter_AFT__A500.DeviceDesc%=SangomaVirtualAdapter_BRI,    CommsAdapter\SangomaAdapter_A500__BRI

;***************************************************************************************
[SangomaVirtualAdapter.NT]
Characteristics	= 0x81	; NCF_VIRTUAL | NCF_HAS_UI
AddReg		    = sang_virtual_if_enum.reg.Common, sang_virtual_if_enum.reg.Media_T1
CopyFiles		= Drivers_Dir, system32.CopyFiles
BusType			= 15	; PNPBus

[SangomaVirtualAdapter.NT.Services]
AddService = sdladrv, %SPSVCINST_ASSOCSERVICE%, sdladrv_Service_Inst

;***************************************************************************************
[SangomaVirtualAdapter_Analog.NT]
Characteristics	= 0x81	; NCF_VIRTUAL | NCF_HAS_UI
AddReg		    = sang_virtual_if_enum.reg.Common, sang_virtual_if_enum.reg.Media_Analog
CopyFiles		= Drivers_Dir, system32.CopyFiles
BusType			= 15	; PNPBus

[SangomaVirtualAdapter_Analog.NT.Services]
AddService = sdladrv, %SPSVCINST_ASSOCSERVICE%, sdladrv_Service_Inst

;***************************************************************************************
[SangomaVirtualAdapter_ADSL.NT]
Characteristics	= 0x81 ; NCF_VIRTUAL | NCF_HAS_UI
AddReg		    = sang_virtual_if_enum.reg.Common, sang_virtual_if_enum.reg.Media_ADSL
CopyFiles		= Drivers_Dir, system32.CopyFiles
BusType			= 15	; PNPBus

[SangomaVirtualAdapter_ADSL.NT.Services]
AddService = sdladrv, %SPSVCINST_ASSOCSERVICE%, sdladrv_Service_Inst

;***************************************************************************************
[SangomaVirtualAdapter_56k.NT]
Characteristics	= 0x81 ; NCF_VIRTUAL | NCF_HAS_UI
AddReg		    = sang_virtual_if_enum.reg.Common, sang_virtual_if_enum.reg.Media_56k
CopyFiles		= Drivers_Dir, system32.CopyFiles
BusType			= 15	; PNPBus

[SangomaVirtualAdapter_56k.NT.Services]
AddService = sdladrv, %SPSVCINST_ASSOCSERVICE%, sdladrv_Service_Inst

;***************************************************************************************
[SangomaVirtualAdapter_BRI.NT]
Characteristics	= 0x81 ; NCF_VIRTUAL | NCF_HAS_UI
AddReg		    = sang_virtual_if_enum.reg.Common, sang_virtual_if_enum.reg.Media_ISDN_BRI
CopyFiles		= Drivers_Dir, system32.CopyFiles
BusType			= 15	; PNPBus

[SangomaVirtualAdapter_BRI.NT.Services]
AddService = sdladrv, %SPSVCINST_ASSOCSERVICE%, sdladrv_Service_Inst

;***************************************************************************************
[sang_virtual_if_enum.reg.Common]
;***************************************************************************************
HKR, , DeviceName,		0,	"\Device\sdladrv"
HKR, , EnumPropPages32,	,	"sdlacfg.dll,EnumPropPages"
HKR, , Icon,			,	"0"

;***************************************************************************************
; Port Driver default configuration
;
HKR, , LogErrors,  				0, "1"  ;1 - Log errors, 0 - do not log
HKR, , SerialNumbersRange,  	0, "0"	;For the first start use, will be changed by the driver.
HKR, , UserWanpipeNumber,		0, "0"	;If "0" - Automatic number assignment, based on "last_serial_number_range" written by
										; "SngBus.sys" in "HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\busenum".
										; If a number between 1 and 128, then user provided it.
HKR, , ExternalSynchronization, 0, "0"	;Off (IN). Use internal Oscillator (default).
HKR, , StartPortWhenComputerStartsFlag, 0, "1"	;WANOPT_YES
HKR, , BufferMultiplierFactor,	0, "1"
HKR, , tdmv_law,				0, "2" 	;default for all types of cards WAN_TDMV_MULAW
HKR, , HWEC_CLKSRC, 			0, "0"	;WANOPT_NO
HKR, , HWEC_NOISE_REDUCTION,	0, "0"	;WANOPT_NO
HKR, , TDMV_DCHAN,				0, "0"	;dchan not used

;************************************************
;******* single Group of channels, default settings:
HKR,,	Media,	     						0,	"0" 		;WAN_MEDIA_NONE
HKR,,	aft_number_of_logic_channels,		0, 	"1"
HKR,,	aft_logic_channel_0_active_ch,		0, 	"1"	
HKR,,	aft_logic_channel_0_line_mode,		0, 	"BitStream"	;do NOT use HDLC as default to avoid CRC error interrupts during install
HKR,,	aft_logic_channel_0_mtu,			0, 	"160"
HKR,,	aft_logic_channel_0_operational_mode,0, 	"API"		;general API, not Voice API
HKR,,	aft_logic_channel_0_idle_char,		0, 	"255"		;0xFF
HKR,,	ClkRefPort, 						0, 	"0"			;0 means no reference port
;E1 only but set a default in case user switches to E1
HKR,,	E1Signalling,						0,	"1"		;E1 CCS
HKR,,	HighImpedanceMode,					0,	"0"		;Off - WANOPT_NO
;Receiver Sensitivity (Max Cable Loss Allowed)
HKR,,	TE_RX_SLEVEL,						0,	"120"	;WAN_TE1_RX_SLEVEL_12_DB
HKR,,	TE_IGNORE_YEL,						0,	"0"		;WANOPT_NO

HKR,,	FE_TXTRISTATE,						0,	"0"	;WANOPT_NO

;Serial AFT A140 default settings - Start
HKR,,	serial_connection_type,		0,	"0"	;WANOPT_PERMANENT
HKR,,	serial_line_coding,			0,	"0"	;WANOPT_NRZ
HKR,,	serial_line_idle,			0,	"0"	;WANOPT_IDLE_FLAG
HKR,,	clock_source,				0,	"0"	;WANOPT_EXTERNAL
HKR,,	Baudrate,					0,	"0"	;64000 - a baud rate in bits per second
;Serial AFT A140 default settings - End

;******* End of common defaults *******
;************************************************


[sang_virtual_if_enum.reg.Media_T1]
;***************************************************************************************
; T1 Media Configuration Defaults - Start
HKR,,Media,			0,	"1"	;T1
HKR,,LDecoding,		0,	"2"	;B8ZS
HKR,,Framing,		0,	"1"	;ESF
HKR,,ClkMode,		0,	"1"	;Normal
HKR,,LBO,			0,	"1"	;0dB
HKR,,tdmv_law,		0,	"2"	;WAN_TDMV_MULAW
; T1 Media Configuration Defaults - End

[sang_virtual_if_enum.reg.Media_E1]
;***************************************************************************************
; E1 Media Configuration Defaults - Start
HKR,,Media,			0,	"2"	;E1
HKR,,LDecoding,		0,	"2"	;HDB3
HKR,,Framing,		0,	"4"	;CRC4
HKR,,ClkMode,		0,	"1"	;Normal
HKR,,LBO,			0,	"1"	;0dB
HKR,,E1Signalling,	0,	"1"	;E1 CCS
HKR,,tdmv_law,		0,	"1" ;WAN_TDMV_ALAW
; E1 Media Configuration Defaults - End

;***************************************************************************************
[sang_virtual_if_enum.reg.Media_Analog]
;***************************************************************************************
; Analog Media Configuration Defaults - Start
HKR,,Media,	     						0, "8" 		;FXO/FXS Analog
HKR,,tdmv_law,							0, "2" 		;WAN_TDMV_MULAW
HKR,,aft_logic_channel_0_mtu,			0, "160"	;default length for Analog - provides 20Ms timing
HKR,,aft_logic_channel_0_operational_mode,	0, "TDM_CHAN_VOICE_API"	;overwrite what was written by 'reg.Common'!!
HKR,,remora_fxo_operation_mode_name,	0, "FCC"	;FCC - is default == TDMV_OPERMODE
HKR,,RM_BATTTHRESH,						0, "3"
HKR,,RM_BATTDEBOUNCE,					0, "16"
HKR,,RM_FXO_TAPPING,					0, "0"		;Off - WAN_RM_DEFAULT == RM_MODE
HKR,,RM_FXO_TAPPING_OFF_HOOK_THRESHOLD,	0, "10" 	;valid values between 5 and 20 == RM_OHTHRESH
HKR,,RM_LCM,							0, "0"		;Off - FXO Loop Current Monitoring is off by default

HKR,,RM_FASTRINGER,						0, "0"		;WANOPT_NO
HKR,,RM_LOWPOWER,						0, "0"		;WANOPT_NO
HKR,,RM_FXSTXGAIN,						0, "0"		;a value
HKR,,RM_FXSRXGAIN,						0, "0"		;a value
HKR,,RM_FXOTXGAIN,						0, "0"		;a value
HKR,,RM_FXORXGAIN,						0, "0"		;a value
HKR,,RM_PULSEDIALING,					0, "0"		;WANOPT_NO
HKR,,RM_RINGAMPL,						0, "0"		;a value
HKR,,RM_RELAXCFG,						0, "0"		;WANOPT_NO
HKR,,RM_FAKE_POLARITY,					0, "0"		;WANOPT_NO
; Analog Media Configuration Defaults - End

;***************************************************************************************
[sang_virtual_if_enum.reg.Media_56k]
;***************************************************************************************
; AFT 56k Media Configuration Defaults - Start
HKR,,Media,	     			0, "3" 		;WAN_MEDIA_56K
HKR,,electrical_interface,	0, "1"		;WANOPT_V35
HKR,,clock_source,			0, "0"		;WANOPT_EXTERNAL
HKR,,BaudRate,				0, "0"		;the line speed, if Internal clock
; AFT 56k Media Configuration Defaults - End

[sang_virtual_if_enum.reg.Media_ISDN_BRI]
;***************************************************************************************
; ISDN_BRI Media Configuration Defaults - Start
HKR,, Media,				0, "9"		;WAN_MEDIA_BRI		0x09
HKR,, tdmv_law,				0, "1"		;WAN_TDMV_ALAW
HKR,, aft_bri_clock_mode,	0, "1"		;WAN_NORMAL_CLK

;************************************************
;******* Three Groups of channels, default settings:
HKR, , aft_number_of_logic_channels,	0, 		"1"		;Two Voice channels and one D-channel. The D-channel interface will be created AUTOMATICALLY by the driver!
;group 0. B-channel 0.
HKR, , aft_logic_channel_0_active_ch,	0, 		"1-2"	;the voice channels
HKR, , aft_logic_channel_0_line_mode,	0, 		"BitStream"
HKR, , aft_logic_channel_0_mtu,			0, 		"160"	;provides 20Ms timing
HKR, , aft_logic_channel_0_operational_mode,0, 	"TDM_CHAN_VOICE_API"	;overwrite what was written by 'reg.Common'!!
																		;Note that on B700 both Analog and BRI lines are in the SAME mode - the TDM_CHAN_VOICE_API mode. Otherwize the card will not work.
HKR, , aft_logic_channel_0_idle_char,	0, 		"255"	;0xFF - required by ISDN BRI as idle char

;************************************************
HKR, , ClkRefPort, 						0, 		"0"	;0 means no reference port
; ISDN_BRI Media Configuration Defaults - End

;***************************************************************************************
[sang_virtual_if_enum.reg.Media_ADSL]
;***************************************************************************************
; ADSL Configuration Defaults - Start
HKR,,Media,	     		0, "0" 		;WAN_MEDIA_NONE
HKR,,electrical_interface,	0, "1"	;WANOPT_V35
HKR,,clock_source,		0, "0"		;WANOPT_EXTERNAL
HKR,,BaudRate,			0, "0"		;the line speed, if Internal clock

;---------------------------------------------------------------------------------------
HKR,,AdslEncapMode,		0, "0" 		;RFC_MODE_BRIDGED_ETH_LLC
;HKR,,AdslEncapMode,		0, "2" 		;RFC_MODE_ROUTED_IP_LLC

HKR,,AdslVpi,	     		0, "0" 		;
HKR,,AdslVci,	     		0, "35"		;

HKR,,AdslVerbose,     		0, "1" 		;

HKR,,AdslRxBufferCount,		0, "50"		;
HKR,,AdslTxBufferCount,		0, "50"		;

;---------------------------------------------------------------------------------------
HKR,,AdslStandard,     		0, "4" 		;WANOPT_ADSL_MULTIMODE
HKR,,AdslTrellis,     		0, "32768"	;WANOPT_ADSL_TRELLIS_ENABLE == 0x8000
HKR,,AdslTxPowerAtten, 		0, "0" 		;
HKR,,AdslCodingGain,   		0, "65280"	;WANOPT_ADSL_AUTO_CODING_GAIN == 0xFF00
HKR,,AdslMaxBitsPerBin,		0, "15"		;== 0xE;
		 
;---------------------------------------------------------------------------------------
HKR,,AdslTxStartBin,	 	0, "6" 		;== 0x6
HKR,,AdslTxEndBin,     		0, "31"		;== 0x1F
		 
;---------------------------------------------------------------------------------------
HKR,,AdslRxStartBin,   		0, "32"		;== 0x20
HKR,,AdslRxEndBin,    		0, "255"	;== 0xFF

;---------------------------------------------------------------------------------------
HKR,,AdslRxBinAdjust,  		0, "0" 		;WANOPT_ADSL_RX_BIN_DISABLE == 0x00
HKR,,AdslFramingStruct,		0, "3" 		;WANOPT_ADSL_FRAMING_TYPE_3 == 0x0003

;---------------------------------------------------------------------------------------
HKR,,AdslExpandedExchange,	0, "32768"	;WANOPT_ADSL_EXPANDED_EXCHANGE == 0x8000
HKR,,AdslClockType,    		0, "4" 		;WANOPT_ADSL_CLOCK_CRYSTAL == 0x04
HKR,,AdslMaxDownRate, 		0, "8192"	;
		 
;---------------------------------------------------------------------------------------
HKR,,aft_logic_channel_0_mtu,		  0,    "1500"	;overwrite what was written by 'reg.Common'!!
HKR,,aft_logic_channel_0_operational_mode,0, 	"STACK" ;overwrite what was written by 'reg.Common'!!

HKR,,Adsl_atm_watchdog,		0, "0" 		;

;---------------------------------------------------------------------------------------
HKR,,AdslRxCellCount,  		0, "1" 		;The minimum - for 64kbs line.
						;Controls the latency of rx interrupt.
; ADSL Configuration Defaults - End

[sdladrv_Service_Inst]
DisplayName    = %sdladrv.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\sdladrv.sys
LoadOrderGroup = Extended Base

[Drivers_Dir]
sdladrv.sys

[system32.CopyFiles]
sdlacfg.dll
wanpipemon.exe
stail.exe
wan_xilinx_test.exe
wan_aftup.exe
wanec_client.exe
stelephony.dll
libsangoma.dll
waneclib.dll
wanrouter.exe
wancfglib.dll

[Strings]
SPSVCINST_ASSOCSERVICE 	= 0x00000002
V_Sangoma	           	= "Sangoma Technologies"
DiskId1					= "Sangoma Installation Disk"
ClassName				= "Sangoma Communications Devices"

;============================================================================================
;
; BIG NOTE: The "Sangoma Hardware Abstraction Driver" string is used by software to search for
;		Sangoma Ports (libsangoma.c and others).  That means this string should not be
;		modified without a VERY good reason.
;
;S518
SangomaVirtualAdapter_AFT__ADSL.DeviceDesc = "  Sangoma Hardware Abstraction Driver (ADSL)"
;A101/A102/A104/A108/A116/T116,  A056  and  A140 :
SangomaVirtualAdapter_AFT_Line1.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 1)"
SangomaVirtualAdapter_AFT_Line2.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 2)"
SangomaVirtualAdapter_AFT_Line3.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 3)"
SangomaVirtualAdapter_AFT_Line4.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 4)"
SangomaVirtualAdapter_AFT_Line5.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 5)"
SangomaVirtualAdapter_AFT_Line6.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 6)"
SangomaVirtualAdapter_AFT_Line7.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 7)"
SangomaVirtualAdapter_AFT_Line8.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 8)"
SangomaVirtualAdapter_AFT_Line9.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 9)"
SangomaVirtualAdapter_AFT_Line10.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 10)"
SangomaVirtualAdapter_AFT_Line11.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 11)"
SangomaVirtualAdapter_AFT_Line12.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 12)"
SangomaVirtualAdapter_AFT_Line13.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 13)"
SangomaVirtualAdapter_AFT_Line14.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 14)"
SangomaVirtualAdapter_AFT_Line15.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 15)"
SangomaVirtualAdapter_AFT_Line16.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Port 16)"
;all Analog Ports:
SangomaVirtualAdapter_AFT__A200.DeviceDesc = "  Sangoma Hardware Abstraction Driver (Analog)"
;all ISDN BRI Ports:
SangomaVirtualAdapter_AFT__A500.DeviceDesc = "  Sangoma Hardware Abstraction Driver (ISDN BRI)"

sdladrv.SVCDESC        = "Sangoma Hardware Abstraction driver"
