SS7 Circuit Report Column Headings

| **Heading** | **Definition** |
| --- | --- |
| **chan** | Timeslot in E1 or T1. ss7boost timeslot numbers begin with 0. Add 1 to get the customary timeslot number. |
| **cfg** | Channel configured for voice. (y/n) |
| **inuse** | Channel being used. (y/n) |
| **inrst** | Channel in process or waiting to be reset. (y/n) |
| **rhb** | Channel is blocked remotely for hardware reasons. (y/n) |
| **lhbs** | Channel is blocked locally because the signal gateway heartbeat is missing. (y/n) |
| **lhbm** | Channel is blocked locally because the media gateway heartbeat is missing. (y/n) |
| **lhbc** | Channel is blocked locally because the E1 or T1 carrying the channel is not connected. (y/n) |
| **lhbr** | Channel is blocked locally because the SS7 route to the remote channel controller is not available. (y/n) |
| **rmb** | Channel is blocked remotely because the channel is manually blocked at remote channel controller. (y/n) |
| **lmb** | Channel is blocked locally because the channel is manually blocked using the ./ss7boost\_cli --ckt-block command. (y/n) |