Dialogic Media Gateway Release Notes

INFORMATION IN THIS DOCUMENT IS PROVIDED IN CONNECTION WITH PRODUCTS OF DIALOGIC CORPORATION OR ITS SUBSIDIARIES (“DIALOGIC”). NO LICENSE, EXPRESS OR IMPLIED, BY ESTOPPEL OR OTHERWISE, TO ANY INTELLECTUAL PROPERTY RIGHTS IS GRANTED BY THIS DOCUMENT. EXCEPT AS PROVIDED IN A SIGNED AGREEMENT BETWEEN YOU AND DIALOGIC, DIALOGIC ASSUMES NO LIABILITY WHATSOEVER, AND DIALOGIC DISCLAIMS ANY EXPRESS OR IMPLIED WARRANTY, RELATING TO SALE AND/OR USE OF DIALOGIC PRODUCTS INCLUDING LIABILITY OR WARRANTIES RELATING TO FITNESS FOR A PARTICULAR PURPOSE, MERCHANTABILITY, OR INFRINGEMENT OF ANY INTELLECTUAL PROPERTY RIGHT OF A THIRD PARTY.
Dialogic products are not intended for use in medical, life saving, life sustaining, critical control or safety systems, or in nuclear facility applications.
Dialogic may make changes to specifications, product descriptions, and plans at any time, without notice.
Dialogic is a registered trademark of Dialogic Corporation. Dialogic's trademarks may be used publicly only with permission from Dialogic. Such permission may only be granted by Dialogic’s legal department at 9800 Cavendish Blvd., 5th Floor, Montreal, Quebec, Canada H4M 2V9. Any authorized use of Dialogic's trademarks will be subject to full respect of the trademark guidelines published by Dialogic from time to time and any use of Dialogic’s trademarks requires proper acknowledgement.
Microsoft is a registered trademark in the United States and/or other countries. Other names of actual companies and products mentioned herein are the trademarks of their respective owners. Dialogic encourages all users of its products to procure all necessary intellectual property licenses required to implement their concepts or applications, which licenses may vary from country to country.

Release 6.0 SU7

November 17, 2010

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.SU7.0.004.app | Gateway Application | |6.0.SU7.0.004|
T1E1_MR17_7.msd | DSP Firmware | |T1E1_MR17_7|
t1e1_6.0.SU7.0.004.fsh | Main CPU Boot | |6.0.SU7.0.004|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.SU7.0.004.app | Gateway Application | |6.0.SU7.0.004|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.SU7.0.004.fsh | Main CPU Boot | |6.0.SU7.0.004|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.SU7.0.004.app | Gateway Application | |6.0.SU7.0.004|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.SU7.0.004.fsh | Main CPU Boot | |6.0.SU7.0.004|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.SU7.0.004.app | Gateway Application | |6.0.SU7.0.004|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.SU7.0.004.fsh | Main CPU Boot | |6.0.SU7.0.004|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.SU7.0.004.app | Gateway Application | |6.0.SU7.0.004|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.SU7.0.004.fsh | Main CPU Boot | |6.0.SU7.0.004|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Added Features:

FR # | Dialogic® Media Gateway Model | Description
5492 | DMG2xxxDTIx | Added support for parsing proprietary information for redirect number for the Avaya MSI integration.
5304 | ALL | Added support for Multi-Part MIME SIP Messages.
5271 | DMG2xxxDTIx | Added support for Calling Line Identification.

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00075358 | ALL | A blind transfer is completed on an ALERTing message and should be completed on a CONNECTed message.
IPY00075458 | ALL | If an INVITE is sent without SDP, then audio is never transmitted on the call.
IPY00075461 | DMG2xxxDTIx | SIP→SIP T.38 calls using tel event payload 101 no longer work after upgrading a Gateway to 6.0 SU6.
IPY00075453 | ALL | In some cases in the contact header the remote phone number was used to build the URI instead of the local phone number.
IPY00075446 | DMG2xxxDTIx | The use of Octet 3.1 is not allowed for QSIG. NOTE: the QSIG ECMA 143 Specification states that the Octet 3.1 should never be set, the Gateway validation has been relaxed to accommodate this PBX.
IPY00075482 | DMG1008DNI | Call are not being answered on a transfer because of delayed lamp updates from the PBX.
IPY00075429 | DMG2xxxDTIx | Voice gets distorted when a hold/unhold is done.
IPY00075507 | ALL | Outbound calls to certain mobile network providers fail.
IPY00075492 | ALL | Aborting a transfer tears down all calls on the transfer.
IPY00075367 | ALL | The Gateway does not parse the CPID information correctly if there is a "9" in the CPID.
IPY00075536 | ALL | A software fault may occur on the Gateway when a message is received by the Gateway that is not associated with an existing dialog.
IPY00075503 | DMG2xxxDTIx | Intermittently on TDM bridged calls the called party cannot hear the caller.
IPY00075445 | DMG2xxxDTIx | The Gateway reports a failure for MWI Clear/Set TDM test on a Tadiran Coral IPX Office with T1-QSIG even though the test actually passes.
IPY00075566 | DMG2xxxDTIx | A conference call from a soft IP client to a PSTN phone times out prematurely.
IPY00075552 | DMG2xxxDTIx | The Gateway disconnects an ISDN→OCS call during ongoing communication.
IPY00075460 | DMG2xxxDTIx | The Gateway does not disconnect on a FACILITY message when connected to an external PSTN call on an Alcatel OmniPCX PBX.
IPY00074573 | DMG2xxxDTIx | The Gateway generates an unexpected "Error _isdnLiFreeTdmChannel(10) already free" error message.
IPY00075575 | DMG2xxxDTIx | The Gateway fails to parse re-direct information in the SETUP message it receives from a Nortel CS1000-NI2.
IPY00075576 | DMG2xxxDTIx | The Gateway fails to parse re-direct information from a SETUP message it receives from DMS100 protocol.
IPY00075545 | DMG2xxxDTIx | The Gateway does not send RTPEvent(Start) to SIPEnd point when sending DTMF via RFC2833.
IPY00075425 | DMG2xxxDTIx | RFC2833 DTMF is not passed to the second leg of a SIP→SIP transcoded call.
IPY00075569 | DMG2xxxDTIx | When switching to T.38 mode in the Gateway the packet time is not cleared or validated and the last existing packet time is used.
IPY00075582 | ALL | The value for max ptime is being misinterpreted as ptime.
IPY00075487 | ALL | The Gateway is not using the redirect information from an inbound SIP call.
IPY00075599 | DMG2xxxDTIx | The gateway may fail to respond to an unhold re-INVITE.

Known Issues:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074278 | ALL | In fax pass-through mode, the Gateway does not notify the VoIP endpoint that it has switched from an LBR codec to G.711.
IPY00074405 | DMG2xxxDTIx | After rebooting certain E1 PBX switches, the E1 span does not recover until the Gateway is rebooted.
IPY00074752 | ALL | The "countryName" parameter associated with CA Signed Certificates can only be two characters long.
IPY00074879 | ALL | When a "&" is contained in the subject field, the Gateway generates a Data_ReadXmlIntoVars() error.
IPY00075293 | DMG1008DNI | The Gateway is not dialing the extension after an FAC for an MWI request.
IPY00074997 | ALL | The Gateway does not carry the authentication state across renegotiation requisition.
IPY00075156 | DMG100xLS | Serial MWIs do not work for NEC 2000 IPS.
IPY00075463 | ALL | Occasionally SIP Continuation is sent in the packet after an ACK.
IPY00075642 | ALL | If a SIP message is sent with Content-Type:application/sdp and no body is sent, the message will be rejected with "406 Not Accepted Here" reply from the Gateway.
IPY00075639 | DMG2xxxDTIx | When using the Remote-Part-ID method of Calling Line Identity, the value of "Name Restricted" from the TDM layer is not passed to SIP layer.
IPY00075620 | DMG2xxxDTIx | For an ISDN→SIP call, the ISDN connection is dropped after four rings even if nobody has answered the SIP endpoint.
IPY00075651 | DMG1008DNI | If an INFO message for a display change is sent to some voicemail applications, the call will be disconnected.
IPY00075614 | DMG1008DNI | If a TDM call on the Gateway terminates quickly, the Gateway port does not clean up properly and will not handle subsequent calls properly.
IPY00075648 | ALL | Memory usage alarms are generated unexpectedly on the Gateway.

Release 6.0 SU6

July 20, 2010

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.SU6.0.004.app | Gateway Application | |6.0.SU6.0.004|
T1E1_MR17_6.msd | DSP Firmware | |T1E1_MR17_6|
t1e1_6.0.SU6.0.004.fsh | Main CPU Boot | |6.0.SU6.0.004|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.SU6.0.004.app | Gateway Application | |6.0.SU6.0.004|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.SU6.0.004.fsh | Main CPU Boot | |6.0.SU6.0.004|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.SU6.0.004.app | Gateway Application | |6.0.SU6.0.004|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.SU6.0.004.fsh | Main CPU Boot | |6.0.SU6.0.004|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.SU6.0.004.app | Gateway Application | |6.0.SU6.0.004|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.SU6.0.004.fsh | Main CPU Boot | |6.0.SU6.0.004|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.SU6.0.004.app | Gateway Application | |6.0.SU6.0.004|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.SU6.0.004.fsh | Main CPU Boot | |6.0.SU6.0.004|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Added Features:

FR # | Dialogic® Media Gateway Model | Description
5129 | DMG2xxxDTIx | Added support for the Gateway to handle digits sent from switches that use overlapped sending for sending digits.
5110 | DMG1xxx | Added support to the DMG1xxx to allow SRTP with 20 ms calls. An 8 port Gateway will be limited to 4 ports when these options are selected.
4033 | ALL | Added support for the Gateway to detect and route fax calls to a single number.
5109 | ALL | Increased the maximum number of available VoIP Host Groups from 10 to 120.
5278 | DMG2xxxDTIx | Included ISDN Progress Indication and Cause Code information in a 183 SIP message.

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074995 | ALL | If a BYE message is sent to the transfer target in the middle of a supervised transfer, subsequent calls will receive an "Error mediaSessionStart() failed -11" message.
IPY00075103 | ALL | For TDM→TDM calls in front of the PBX, a STATUS message is sent to the PBX if a NOTIFY is sent to the Gateway during a call which causes the call to drop.
IPY00075133 | ALL | Calls through the Gateway are not integrated correctly on some occasions.
IPY00075088 | DMG2xxxDTIx | A VoIP→VoIP transfer fails with reason "Service Unavailable".
IPY00075056 | DMG2xxxDTIx | Ports on a T1 CAS integration do not free up if the next call comes in too quickly after the previous call disconnects.
IPY00075131 | ALL | The Gateway is not able to strip a prefix for an international call (011) and send the call out with call type information of international.
IPY00075152 | ALL | DNS lookup on the Gateway does not support CNAME.
IPY00075147 | ALL | When a change is made at the end of the CPID table and the config.ini file is exported, an extra space is present and the config.ini cannot be imported.
IPY00074727 | ALL | The Gateway does not support the use of a ">" sign in a name of a route rule.
IPY00075201 | ALL | An unexpected CLeg Not Found alarm is generated.
IPY00075122 | DMG2xxxDTIx | The Gateway's state remains off hook when a timeout occurs waiting for a WINK.
IPY00075187 | ALL | The Gateway is not able to parse an INVITE with a tel tag in the request URI field: INVITE tel:+XXXX.
IPY00075196 | ALL | Echo cancellation parameters are not available through the web interface.
IPY00074969 | ALL | Payload type for outbound calls is not configurable.
IPY00075205 | ALL | The Gateway generates a "Transaction Not Found" alarm when it receives a "302 Moved Temporarily" and the TDM disconnects.
IPY00075211 | ALL | The Gateway is replacing "#" with "%23".
IPY00075264 | ALL | Supervised transfer call fails when the INVITE contains a Transfer-From header.
IPY00075295 | ALL | The Gateway is not playing A, B, C, or D DTMF within a SIP INFO message.
IPY00075264 | DMG1008DNI | The Gateway unexpectedly disconnects the primary call on a supervised transfer.
IPY00075334 | ALL | In some situations, MWIs would fail and generate "Command MWI Timed Out: Success" error.
IPY00075335 | ALL | B-Channel assignment fails when DMG is in Network Mode.
IPY00075279 | ALL | The Gateway sends the ISDN Redirect number in the SIP header 'Diversion' field.
IPY00075279 | ALL | Formatting of the ISDN Redirect number in the SIP header causes SR140 to not pick up the redirect number.

Known Issues:

Defect # | Dialogic® Media Gateway Model | Description
IPY00075429 | DMG2xxxDTIx | After the re-INVITE for an un-hold, there is no voice or garbled voice between the two endpoints.
IPY00074278 | ALL | In fax pass-through mode, the Gateway does not notify the VoIP endpoint that it has switched from an LBR codec to G.711.
IPY00074405 | DMG2xxxDTIx | After rebooting certain E1 PBX switches, the E1 span does not recover until the Gateway is rebooted.
IPY00075425 | DMG2xxxDTIx | DTMF is not correctly passed to the second leg of the call when transcoding is required.
IPY00074257 | ALL | All SIP messages are parsed even if it flagged as truncated.
IPY00074611 | ALL | An INTERNAL ERROR is generated when an INFO message and a REFER message are received simultaneously.
IPY00074687 | DMG2xxxDTIx | The Gateway experiences a software fault and restarts.
IPY00075445 | DMG2xxxDTIx | The Gateway reports "Device Not Available" even though the MWI light changes states when connected to a Tadiran Coral IPx Office via T1-QSIG.
IPY00074752 | ALL | The "countryName" parameter associated with CA Signed Certificates can only be two characters long.
IPY00074879 | ALL | When a "&" is contained in the subject field, the Gateway generates a Data_ReadXmlIntoVars() error.
IPY00075367 | DMG100xLS | CPID is not parsed correctly when using the rule "9\d(2-10).
IPY00075293 | DMG1008DNI | The Gateway is not dialing the extension after an FAC for an MWI request.
IPY00074997 | ALL | The Gateway does not carry the authentication state across renegotiation requisition.
IPY00075358 | DMG2xxxDTIx | The Gateway is completing a transfer before the complete is expected.
IPY00075156 | DMG100xLS | Serial MWIs do not work for NEC 2000 IPS.

Release 6.0 SU5

February 22, 2010

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.SU5.0.009.app | Gateway Application | |6.0.SU5.0.009|
T1E1_MR17_5.msd | DSP Firmware | |T1E1_MR17_5|
t1e1_6.0.SU5.0.009.fsh | Main CPU Boot | |6.0.SU5.0.009|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.SU5.0.009.app | Gateway Application | |6.0.SU5.0.009|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.SU5.0.009.fsh | Main CPU Boot | |6.0.SU5.0.009|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.SU5.0.009.app | Gateway Application | |6.0.SU5.0.009|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.SU5.0.009.fsh | Main CPU Boot | |6.0.SU5.0.009|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.SU5.0.009.app | Gateway Application | |6.0.SU5.0.009|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.SU5.0.009.fsh | Main CPU Boot | |6.0.SU5.0.009|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.SU5.0.009.app | Gateway Application | |6.0.SU5.0.009|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.SU5.0.009.fsh | Main CPU Boot | |6.0.SU5.0.009|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Added Features:

FR # | Dialogic® Media Gateway Model | Description
3230 | ALL | Added support to allow calls with different codecs to go through the Gateway simultaneously.
3257 | DMG2xxxDTIx | Added support to transcode calls with different codecs.
5222 | DMG2xxxDTIx | Added support for ISDN and Analog modem calls.

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074631 | ALL | When a routing rule is dragged too quickly through the routing table, it will not drop in the expected location.
IPY00074632 | ALL | An INVITE message containing a long URI does not return a 414 response.
IPY00074782 | ALL | The INVITE message sent by the Gateway contains the transport parameter in the contact header but does not bind it to the URI.
IPY00074831 | ALL | The Gateway transmits a zero for an RTP port number for a HOLD re-INVITE on a SIP→SIP call.
IPY00074825 | DMG2xxxDTIx | The Gateway intermittently fails to get the call party ID from the SMDI link on T1 CAS.
IPY00074887 | DMG2xxxDTIx | RED alarm is not debounced per ANSI T1.231.
IPY00074827 | DMG100xLS | The Gateway intermittently fails to get the call party ID from the SMDI link on Analog.
IPY00074813 | ALL | The Gateway drops calls when inter-networking ISDN progress messages are present.
IPY00074888 | DMG2xxxDTIx | A Gateway TDM channel may hang if a second incoming ISDN ALERT message was received.
IPY00074790 | DMG2xxxDTIx | The configuration parameter srtpUnEncryptedSRTCP is not available via the web interface.
IPY00074715 | DMG1008DNI | Added support for digital answer supervision on Nortel PBXs.
IPY00074876 | ALL | Gateway Software Fault - Hardware Watchdog Expiration: Warm Reset was experienced on the Gateway.
IPY00074864 | DMG2xxxDTIx | Hook flash transfers that are aborted cause the T1 CAS port to hang.
IPY00074781 | DMG2xxxDTIx | The Gateway disconnects a call when a PROG message is received with an unsupported IE.
IPY00074829 | DMG2xxxDTIx | For TDM→TDM calls the ISDN call type information is not passed from the inbound call to the outbound call.
IPY00074882 | ALL | Some supervised transferred calls will cause the port on the Gateway to no longer take incoming calls.
IPY00074832 IPY00074885 | DMG2xxxDTIx | The Gateway is disconnecting CAS when a proprietary distinctive ring feature is enabled on the switch side.
IPY00074902 | ALL | Gateway gets into a state where it responds to all Options messages with 503 Service Unavailable.
IPY00074871 | ALL | When the Gateway sends a REGISTRATION message, the user id is not included in the contact binding field.
IPY00074624 | ALL | Reception of multiple REFER messages for a single call is not supported.
IPY00074828 | ALL | For supervised transfer when the first TDM call leg disconnects, the Gateway disconnects the second call leg as well.
IPY00074907 | DMG2xxxDTIx | Fax calls fail when the exclusive bit in the Bearer Capabilities IE is not enabled.
IPY00074867 | DMG1008DNI | DMG1000 ports are going in and out of service on Nortel.
IPY00074768 | ALL | Certain outbound fax calls from the Gateway get rejected with a reason of incompatible destination.
IPY00074909 | DMG2xxxDTIx | If an INVITE to the Gateway has no SDP, the call will be connected with no media.
IPY00074757 | ALL | Added support for SIP transport change via refer-to header.
IPY00074945 | DMG2xxxDTIx | When a P-asserted Identity header is set with user=phone the call is dropped.
IPY00074972 | DMG2xxxDTIx | The Gateway does not support inbound ISDN calls with unrestricted digital information bearer capability.

Known Issues:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074450 | DMG1xxxLS | Gateway does not always disconnect a call when a disconnect tone is received.
IPY00074278 | ALL | In fax pass-through mode, the Gateway does not notify the VoIP endpoint that it has switched from an LBR codec to G.711.
IPY00074405 | DMG2xxxDTIx | After rebooting certain E1 PBX switches, the E1 span does not recover until the Gateway is rebooted.
IPY00074589 | ALL | Gateway call log does not match the number of active channels in the TDM status page.
IPY00074501 | ALL | SRTP is allowed to be set up with 20 ms frame size, even if this combination is an invalid setup.
IPY00074257 | ALL | All SIP messages are parsed even if it flagged as truncated.
IPY00074611 | ALL | An INTERNAL ERROR is generated when an INFO message and a REFER message are received simultaneously.
IPY00074687 | DMG2xxxDTIx | The Gateway experiences a software fault and restarts.
IPY00074727 | ALL | If a rule label contains a ">" the name will be changed when submitted.
IPY00074752 | ALL | The "countryName" parameter associated with CA Signed Certificates can only be two characters long.
IPY00074879 | ALL | When a "&" is contained in the subject field, the Gateway generates a Data_ReadXmlIntoVars() error.
IPY00074917 | DMG1008DNI | Remote MWIs fail on Nortel M1, when done between more than one Nortel switch.
IPY00074969 | DMG2xxxDTIx | The Gateway only supports payload type 101 for DTMF on SIP→SIP calls.
IPY00074997 | ALL | The Gateway does not carry the authentication state across renegotiation requisition.
IPY00075031 | DMG2xxxDTIx | When a SIP→SIP call is put on hold, it unexpectedly drops after 30 seconds of holding.
IPY00075147 | ALL | The Gateway creates a space in front of the start of the routing table tag in the xml file if a change is made to the end of the CPID table.
IPY00075156 | DMG100xLS | Serial MWIs do not work for NEC 2000 IPS.
IPY00075180 | DMG2xxxDTIx | For TDM«VoIP calls using codec G.722 on the VoIP side, the voice will sound garbled. This will also be the case for VoIP → VoIP calls if only one side is G.722.

Release 6.0 SU4

July 30, 2009

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.SU4.0.012.app | Gateway Application | |6.0.SU4.0.012|
T1E1_MR17_02.msd | DSP Firmware | |T1E1_MR17_02|
t1e1_6.0.SU4.0.012.fsh | Main CPU Boot | |6.0.SU4.0.012|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.SU4.0.012.app | Gateway Application | |6.0.SU4.0.012|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.SU4.0.012.fsh | Main CPU Boot | |6.0.SU4.0.012|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.SU4.0.012.app | Gateway Application | |6.0.SU4.0.012|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.SU4.0.012.fsh | Main CPU Boot | |6.0.SU4.0.012|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.SU4.0.012.app | Gateway Application | |6.0.SU4.0.012|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.SU4.0.012.fsh | Main CPU Boot | |6.0.SU4.0.012|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.SU4.0.012.app | Gateway Application | |6.0.SU4.0.012|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.SU4.0.012.fsh | Main CPU Boot | |6.0.SU4.0.012|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Added Features:

FR # | Dialogic® Media Gateway Model | Description
3090 | ALL | Add support for SIP Registration and Authentication as both the server and the client.
3292 3423 | DMG2xxxDTIx | Added the ability to support TCP and UDP calls simultaneously.
3542 | ALL | Added support for pre and post feature access codes (FAC) for message waiting indicators (MWI).
3257 | DMG2xxxDTIx | Added the ability to support routing calls from one SIP endpoint to another SIP endpoint.
3491 | ALL | Added support for ISDN call type for TDM → VoIP calls.

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074265 | ALL | TCP Inactivity timer default is too short and will be increased to 90 seconds.
IPY00074511 | DMG2xxxDTIx | Path replacement optimization intermittently fails on Avaya PBX.
IPY00074515 | DMG1008RLMDNIW | Forward Busy calls fail to integrate on the DMG1008RLMDNIW.
IPY00074536 | ALL | A negative number in the learn tone fields generates a non-descript error message.
IPY00074531 | DMG1008MTLDNIW | MWIs fail on the DMG1008MTLDNIW when the FAC is specified in the NOTIFY message instead of the Gateway Configuration interface.
IPY00074569 | ALL | The Gateway is sending Specific Trap = 0 when Specific Trap = 1 is expected for an enterprise level SNMP alarm.
IPY00074590 | ALL | Gateway web interface is not accessible through HTTPS.
IPY00074314 | DMG1xxx | The IP → TDM gain setting on the DMG1xxx models does not affect the DTMF levels in that direction.
IPY00074554 | ALL | A JavaScript warning is given on startup in MSIE8.0.
IPY00074572 | ALL | Gateway generates SIP INFO messages when only the call reason changes.
IPY00074526 | ALL | The Gateway incorrectly converts spaces to %20 characters when sending call name information.
IPY00074602 | ALL | Payload type 13 (comfort noise) is not accepted when VAD is disabled.
IPY00074519 | DMG2xxxDTIx | Routing table only supports 100 entries for Inbound TDM and Inbound VoIP rules.
IPY00074607 | DMG2xxxDTIx | TDM Trunk Groups do not support 120 groups.
IPY00074568 | ALL | Call ID information is not manipulated for a REFER message received for a transfer.
IPY00043917 | ALL | On TDM → VoIP call if the VoIP media session is inactive when the VoIP send a 200OK message, the Gateway never answers the TDM call and never sends an ACK.
IPY00074618 | ALL | Faxes are failing from TDM → VoIP because CED tones are not detected.
IPY00074622 | ALL | The Gateway is not sending # in the dial string.
IPY00074626 | ALL | The SIP TLS server session cache will attempt to cache 20k entries which can cause the web admin pages to load incorrectly or not at all.
IPY00074608 | ALL | When the Gateway’s configuration file is downloaded via BootP and TFTP, some of the configuration settings do not take effect.
IPY00074625 | ALL | TDM → VoIP calls will go RNA when using TLS.
IPY00074678 | DMG2xxxDTIx | The redirecting party information is not in the setup messages for NI2 protocol for VoIP → TDM calls.

Known Issues:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074450 | DMG1xxxLS | Gateway does not always disconnect a call when a disconnect tone is received.
IPY00074278 | ALL | In fax pass-through mode, the Gateway does not notify the VoIP endpoint that it has switched from an LBR codec to G.711.
IPY00074405 | DMG2xxxDTIx | After rebooting certain E1 PBX switches, the E1 span does not recover until the Gateway is rebooted.
IPY00074589 | ALL | Gateway call log does not match the number of active channels in the TDM status page.
IPY00074501 | ALL | SRTP is allowed to be set up with 20 ms frame size, even if this combination is an invalid setup.
IPY00074257 | ALL | All SIP messages are parsed even if it flagged as truncated.
IPY00074611 | ALL | An INTERNAL ERROR is generated when an INFO message and a REFER message are received simultaneously.
IPY00074617 | ALL | When a route rule is dragged through five or more rules to quickly, the drop location is not accurate.
IPY00074620 | ALL | When a transfer is done immediately after going off hook, the switch does not register the hook flash and the transfer request is not accepted.
IPY00074624 | ALL | Multiple, simultaneous REFER messages are not supported by the Gateway.
IPY00074632 | ALL | Long URI addresses within in the INVITE packet cause the Gateway to exception and/or restart.
IPY00074643 | ALL | The Gateway does not properly bind the URI parameters when using brackets "<>".
IPY00074686 | DMG2120DTIx | The Gateway experiences a software fault "VWSS_STSK" and restarts.
IPY00074687 | DMG2xxxDTIx | The Gateway experiences a software fault and restarts.
IPY00074715 | DMG1xxxDNI | There is no out of band answer supervision for the DMG1008DNI.
IPY00074727 | ALL | If a rule label contains a ">" the name will be changed when submitted.
IPY00074751 | ALL | If the PROG message is present, calls using a mediation server will fail when the PBX signals in-band tones availability to the Gateway.
IPY00074768 | DMG2xxxDTIx | Some faxes will fail with incompatible destination if the call is sent as a voice call, but the fax endpoint is expecting data or some other non-voice type call.
IPY00074690 | DMG2xxxDTIx | When more than 100 routing rules are used, there is an increased amount of time to initially load the web interface page.

Release 6.0 SU3.1

May 29, 2009

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.136.app | Gateway Application | |6.0.136|
T1E1_MR17_02.msd | DSP Firmware | |T1E1_MR17_02|
t1e1_6.0.136.fsh | Main CPU Boot | |6.0.136|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.136.app | Gateway Application | |6.0.136|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.136.fsh | Main CPU Boot | |6.0.136|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.136.app | Gateway Application | |6.0.136|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.136.fsh | Main CPU Boot | |6.0.136|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.136.app | Gateway Application | |6.0.136|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.136.fsh | Main CPU Boot | |6.0.136|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.136.app | Gateway Application | |6.0.136|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.136.fsh | Main CPU Boot | |6.0.136|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074484 | DMG2xxxDTIx | Call dropped by the Gateway when the number of digits received is less than the minimum number configured in the Gateway for ISDN Overlapped Receive dialing.
IPY00074442 IPY00074456 | DMG1xxx | Gateway will reboot for dial strings that take longer than 10 seconds to dial.
IPY00074443 | DMG1xxx | The CNG tone is not rendered correctly to the TDM line after a re-INVITE to a T38 session.
IPY00074446 | DMG2xxxDTIx | Nortel Option 11 PBX reports “Calls Barred” for calls from the Gateway when the protocol is DMS100.
IPY00074449 | DMG2xxxDTIx | Caller ID is not passed on TDM → IP on certain Avaya PBXs using T1 QSIG.
IPY00074462 | ALL | Call integration errors on Toshiba integration when the time sync packet is sent from the switch.
IPY00074485 | DMG2xxxDTIx | IP transfer to an external TDM number returns a “488 Not Acceptable Here” message.
IPY00074498 | ALL | The INVITE expiration timeout defined by T1 and T2 SIP timers are inaccurate.
IPY00074502 | ALL | Added support for SIP display names that are not in quotes.
IPY00074503 | ALL | An underscore in the SIP hostname is not supported.
IPY00074508 | DMG2xxxDTIx | Ringback tone generation for various countries is not user configurable.
IPY00074300 | DMG2xxxDTI | The Enable Failover configuration parameter is available to the user on non-survivability models.
IPY00074516 | DMG2xxxDTIx | The Gateway does not generate busy tone when connected via T1 CAS – EM Wink.
IPY00074358 | ALL | When the Gateway receives a REFER request for a transfer while in the waiting for CPID state, the transfer fails.
IPY00074230 | ALL | The Gateway’s web interface does not respond when too many connections are attempted.
IPY00074506 | ALL | Trace messages are sent out the serial port when the Gateway is configured for serial integration.
IPY00074469 | ALL | Calls through the Gateway using T.38 fail for a variety of reasons including – the Gateway includes redundant m=image lines in SDP Answer in response to a fax re-INVITE and the Gateway only includes an m=audio line in SDP Answer response to a fax re-INVITE.
IPY00074509 | DMG2xxxDTIx | The Gateway does not generate busy tone when connected via T1 CAS – EM Wink.
IPY00074470 IPY00074507 | DMG2xxxDTIS | Faxes were not handled using T.38 and a Media session was not starting resulting in faxes failing to transmit.
IPY00074514 | ALL | TDM to TDM faxes do not switch to T.38 on occasion.
IPY00074521 | DMG2xxxDTIx | TDM to TDM routes have audio delays.
IPY00074538 | DMG2xxxDTIx | Inbound TDM calls from PSTN to another TDM device are disconnecting immediately because of a resource leak.
IPY00074537 | DMG2xxxDTIx | A large number of Media Session Open Failed alarms are generated.
IPY00074545 | ALL | The Gateway does not send the media offer for image when in audio mode causing faxes to fail in some instances.
IPY00074528 | DMG2xxxDTIx | The Gateway does not load the ISDN Call Type configuration after a reboot.
IPY00074548 | DMG2xxxLS | An alarm is generated for every in-band MWI on analog.
IPY00074550 | DMG1xxx | T.38 fails if media session is started with SRTP.

Release 6.0 SU3

March 5, 2009

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.128.app | Gateway Application | |6.0.128|
T1E1_MR17_02.msd | DSP Firmware | |T1E1_MR17_02|
t1e1_6.0.128.fsh | Main CPU Boot | |6.0.128|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.128.app | Gateway Application | |6.0.128|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.128.fsh | Main CPU Boot | |6.0.128|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.128.app | Gateway Application | |6.0.128|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.128.fsh | Main CPU Boot | |6.0.128|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.128.app | Gateway Application | |6.0.128|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.128.fsh | Main CPU Boot | |6.0.128|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.128.app | Gateway Application | |6.0.128|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.128.fsh | Main CPU Boot | |6.0.128|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074225 | ALL | The Gateway requires a restart after the quick configuration wizard is run even if none of the options are changed.
IPY00074464 | ALL | When a call is placed on hold via a media level connection, it will not transition properly to unhold.
IPY00074453 | ALL | A memory leak exists if the Gateway receives a response where the local tags do not match the existing dialog.
IPY00074435 | ALL | The Gateway does not reliably include the unsupported media lines in the SDP Answer it sends to a VoIP endpoint.
IPY00074399 | ALL | Trailing spaces in the VoIP→ General Page → Host and Domain fields cause failures for Gateway to fax, specifically, the re-INVITE from the VoIP endpoint to transition to a fax call.
IPY00074431 | DMG2xxxDTIx | The Gateway does not respond to PROGRESS messages with SIP 183 correctly in both TDM→VoIP and VoIP→TDM directions.
IPY00074378 | DMG2xxxDTIx | RTP dynamic payload type 127 is not supported.
IPY00074436 | ALL | The media level connection information is not stored per stream, so when multiple connections are specified, the last connection will apply to all streams.
IPY00074391 | DMS1004LS | Reading registers from the SiLabs chip intermittently gives bad data.
IPY00074289 | DMG2xxxDTIx | For TDM to VoIP calls, the call is dropped when a SIP INFO message tag is not matched.
IPY00074219 | DMG1008LS | Incorrect parsing of CPID from serial interface with Ericsson MD110 when there are leading spaces in the serial message.
IPY00074422 | ALL | The ptime attribute is not being recognized by the Gateway.
IPY00074452 | ALL | The Gateway does not include the client authentication key usage for x509 certificates created by the Gateway. The certificate purpose validation will be a configurable option.
IPY00074420 | DMG2030DTIQ | The E&M Wink settings are not preserved on an upgrade from 5.1 to 6.0.
IPY00074379 | ALL | When an *.ini file in imported to the Gateway, a restart is required regardless of the changes made.
IPY00074451 | ALL | When a G723 offer is made to the Gateway while the Gateway is configured for G711, the Gateway would fail to detect unsupported media.
IPY00074428 | DMG2xxxDTIx | The Gateway does not include unsupported media lines in the SDP Answer sent to the VoIP endpoint.
IPY00074424 | ALL | The “user=phone” parameter is not configurable.
IPY00074417 | DMG2xxxDTIx | The Gateway does not recognize when a T1 line is connected when the T1 line is connected after the Gateway is running.
IPY00074434 | ALL | The Gateway does not send RTCP packets when the call is placed on hold.
IPY00074432 | DMG2xxxDTIx | The Gateway does not respond to ALERTING messages with SIP 180 correctly in both TDM → VoIP and VoIP→TDM directions.
IPY00074315 | DMG2xxxDTIx | The debug trace message “TDM Channel not in use – attempting to free a channel that is already free” is generated after a T1 CAS transfer.
IPY00074365 | DMG2xxxDTIx | Transfers are failing when the switch does indicate ALERTING via the D-channel on ISDN.
IPY00074362 | ALL | The Gateway stops playing ringback tone when an early media session is negotiated.
IPY00074233 | ALL | The name field in the routing table will only accept 39 characters.
IPY00074395 | DMG1xxxLS | The Gateway does not handle CPID when it is sent before the first ring.
IPY00074403 | DMG1008RLM | The Gateway does not process MWI's TDM to IP on Rolm 9751.
IPY00074412 | DMG1xxxLS | A comfort noise packet is being sent when VAD is disabled.
IPY00074302 | DMG2xxxDTIx | There is no option on the Gateway to choose which diverting leg information to use for ISDN calls.
IPY00074401 | ALL | Gateway is sending unsupported media (indicated by setting the port to 0) in SDP offer.
IPY00074375 | ALL | Called name is not displayed properly in the call log when the called name string consists of dialable characters.
IPY00074305 | ALL | When the Gateway finds a mismatch in the codecs a 415 message is sent as the response instead of a SIP 488.
IPY00074363 | ALL | Anonymous calls are not sent with user=phone attribute in the SIP INVITE message.
IPY00074391 | DMG1xxxLS |

Release 6.0 SU2

December 22, 2008

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.121.app | Gateway Application | |6.0.121|
T1E1_MR17_02.msd | DSP Firmware | |T1E1_MR17_02|
t1e1_6.0.121.fsh | Main CPU Boot | |6.0.121|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.121.app | Gateway Application | |6.0.121|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.121.fsh | Main CPU Boot | |6.0.121|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.121.app | Gateway Application | |6.0.121|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.121.fsh | Main CPU Boot | |6.0.121|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.121.app | Gateway Application | |6.0.121|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.121.fsh | Main CPU Boot | |6.0.121|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.121.app | Gateway Application | |6.0.121|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.121.fsh | Main CPU Boot | |6.0.121|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Added Features:

FR # | Dialogic® Media Gateway Model | Description
3378 | ALL | Add configuration option of SRTP_Optional, to allow the gateway to process calls to/from endpoints in either secure or non-secure mode.
3245 | ALL | Add support to provide calling and called type of number (Default, Unknown, International, National, Network Subscriber, Abbreviated or Reserved) and calling and called number plan (Default, Unknown, ISDN_E.164, Data_X.121, Telex_F69, Standard, Private, or Reserved) on a per call basis.

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074224 | All | The Gateway fails to route calls when there are quotes included in the DN Name.
IPY00043928 | DMG2xxxDTIx | When PBX b-channels are taken out of service the telephony page does not reflect the status. This is supported for NI-2, 5ESS and DMS100 only.
IPY00074218 | All | The pass-through fax does not work when the gateway is running in A-Law mode.
IPY00074274 | DMG2xxxDTIx | On a VoIP to TDM call where the TDM side disconnects during call setup a “Server Timeout” error will be generated on the next call.
IPY00044955 | DMG2xxxDTIx | DMG is returning a ''500 INTERNAL SERVER ERROR'' with the Q.931 cause being ''INVALID INFORMATION ELEMENT CONTENTS''.
IPY00074246 | DMG2xxxDTIx | IP side connects when DTMF tones are received on the ISDN side before the ISDN call has been connected. This should be configurable.
IPY00074248 | DMG2xxxDTIx | Gateway reports a red alarm on T1 interface but does not report when the alarm goes back to green.
IPY00074264 | DMG2xxxDTIx | The Gateway is not connecting VoIP to TDM call to a cell phone.
IPY00074267 | All | The web interface to the Gateway fails to render the call log page on occasion.
IPY00074221 | All | During an MWI load test the gateway raises an alarm for being out of RTP ports.
IPY00074299 | DMG2xxxDTIx | T1 QSIG progress message is not parsed correctly.
IPY00074307 | DMG2xxxDTIx | When the Gateway is configured for DMS-100, the outgoing SETUP message is missing the display name included in the INVITE.
IPY00074279 | DMG2060DTISQ | IP Calls to a cell phone via a PBX are failing to complete.
IPY00074277 | DMG2xxxDTIx | After a few weeks the Gateway stops processing calls and must be restarted to recover.
IPY00074321 | ALL | Microsoft OCS - user=phone parameter not supported when the destination is a telephone number on TDM-to-IP calls.
IPY00074303 | ALL | A blank INFO is not being sent if no CPID is received for TDM to IP calls.
IPY00074249 | ALL | Various issues when using FireFox version 2.
IPY00044662 | DMG2xxxDTIx | Media start is failing when interoperating with an SBC (CXC from Convergence).
IPY00074330 | DMG2xxxDTIx | The return cause code of 127 (0x7F) is not sent to TDM when a SIP 487 response is received from the VoIP endpoint.
IPY00074285 | ALL | Calls from TDM to IP do not include the called party number in the INFO message.
IPY00074298 | DMG1004LS | The Gateway is not using the port specified by the port tag in the NOTIFY message.
IPY00078366 | DMG2xxxDTIx | The terminal Vxworks command “task checkstack” causes a data abort on the DMG2000.
IPY00074327 | ALL | VoIP to TDM MWI requests fail if the TDM switch does not provide dialtone.
IPY00074323 | ALL | Gateway sends and receives audio even after offer/answer with a=sendonly or a=rcvonly.
IPY00074326 | ALL | If neither the NAME nor NUMBER of a URI is known 'anonymous' is not used.
IPY00074304 | ALL | IP side connects when DTMF tones are received on the TDM side before the TDM call has been connected for all non-ISDN protocols. This should be configurable.
IPY00074286 | DMG2xxxDTIx | TDM to IP calls cause Gateway to reboot when using serial MCI.
IPY00074331 | DMG2xxxDTIx | A-law and µ-law codecs indicated in SDP response are not simultaneously supported by the DMG2xxx platform.
IPY00074336 | DMG2xxxDTIx | Incoming TDM calls on 4ESS are dropped due to Bearer Capability incompatibilities.
IPY00074340 | ALL | The parameter “gwSigDigitRelay” should default to off.
IPY00074211 | DMG2xxxDTIx | Error message is not generated when all spans on the Gateway are full and a transfer is attempted.
IPY00074322 | DMG2xxxDTIx | Gateway responds with SIP 480 when T1 line is unplugged instead of SIP 503.
IPY00074338 | ALL | There is no parameter to allow users to determine if the Gateway should support reliable provisional responses or not.
IPY00074320 | ALL | Early Media is not supported for TDM-to-IP calls.
IPY00074297 | DMG2xxxDTIx | TIMG resources spike on serial MWI Requests and generate an Error: No free objects.
IPY00074333 | ALL | IP call is not placed on hold when the IP address is 0.0.0.0 on a SIP REINVITE.
IPY00074313 | DMG2xxxDTIx | Transfers are failing due to “Failed to get outbound route”.
IPY00074355 | ALL | Support for the phone=context attribute is not supported. It should be user configurable.
IPY00074345 | DMG2xxxDTIx | Unsupervised transfers on T1 CAS with no FAC, take 6 seconds to complete the transfer.
IPY00074384 | DMG1xxxLS | The TDM port number is not sent in the INVITE when a serial protocol is used to integrate to the TDM network.
IPY00074370 | DMG2xxxDTIx | Load balancing does not use each channel in the VoIP Host Group.
IPY00074348 | DMG2xxxDTIx | Add support for sending Network Specific Facility (NSF) IE for ISDN 5ESS.
IPY00074296 | DMG2xxxDTIx | On a VoIP to TDM call where the TDM side disconnects during call setup a “Server Timeout” error will be generated on the next call in additional scenarios.
IPY00074308 | DMG2xxxDTIx | Gateway would become unresponsive after about 2 weeks of run time and all calls would go ring no answer.
IPY00074326 | DMG1xxx | When the there is no Name or Number information on TDM-to-IP calls, “anonymous” should be used in the INVITE sent to the VoIP endpoint.
IPY00074342 | DMG2xxxDTIx | The presentation indicator byte is not provided in the calling name when a DMS-100 is connected to a NI-1 PSTN switch.
IPY00074343 | ALL | A limited amount of MWIs are executed before the gateway runs out of resources.

Release 6.0 SU1

September 12, 2008

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.110.app | Gateway Application | |6.0.110|
T1E1_MR11.msd | DSP Firmware | |T1E1_MR11|
t1e1_6.0.110.fsh | Main CPU Boot | |6.0.110|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.110.app | Gateway Application | |6.0.110|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.110.fsh | Main CPU Boot | |6.0.110|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.110.app | Gateway Application | |6.0.110|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.110.fsh | Main CPU Boot | |6.0.110|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.110.app | Gateway Application | |6.0.110|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.110.fsh | Main CPU Boot | |6.0.110|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.110.app | Gateway Application | |6.0.110|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.110.fsh | Main CPU Boot | |6.0.110|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Added Features:

FR # | Dialogic® Media Gateway Model | Description
FR2972 | ALL | Added support for transporting DTMF digits between the Gateway and the VoIP endpoints via out-of-band call control messages in SIP.
FR3177 | DMG2xxxDTIx DMG100xLS | Add support for configurable feature code for transfer setup.
FR3031 | DMG2xxxDTIx DMG100xLS DMG1008DNI | Add support for remote disconnect packet on MD110 serial protocol.
FR3181 | DMG2xxxDTIx | Add support for using the CPID from the SIP REFER message on ISDN.
FR3272 | DMG2xxxDTIx | Add support to provide calling and called type of number (Default, Unknown, International, National, Network Subscriber, Abbreviated or Reserved) and calling and called number plan (Default, Unknown, ISDN_E.164, Data_X.121, Telex_F69, Standard, Private, or Reserved) on a per unit basis.

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074252 | All | A space is appended to the end of the common name of a certificate was causing calls to fail when TLS is enabled.
IPY00043905 | DMG1008RLMDNI | The ADEPT parser in the Gateway is not properly interpreting the rules that include a single literal character.
IPY00043403 | All | The Gateway rejects MWI requests that use string "Yes" instead of 'yes' in a NOTIFY message.
IPY00043904 | DMG100xLS | The Gateway incorrectly disconnects a VoIP-to-TDM call when the far end answers the call if the Gateway is connected to a NT1+ device.
IPY00043960 | DMG2xxxDTIx | The Gateway delays starting media after an unsupervised transfer is performed to a TDM destination on a VoIP-to-TDM call when the Gateway is connected to an ISDN protocol.
IPY00043906 | DMG2xxxDTIx | When the Gateway is connected to a Nortel Option 61c / 11c PBX and is configured to use the DMS100 protocol, the user will not be able to make or receive calls due to packet decoding on the D-Channel.
IPY00043967 | DMG2xxxDTIx | No called party is available from IP to TDM when “SIP” is used in the From header because the gateway was case sensitive and did not recognize capitalized “SIP”.
IPY00043909 | All | The Gateway requires a reboot if the user removes the MWI FAC setting. The reboot is required even though the Gateway does not inform the user to reboot.
IPY00043976 | DMG2xxxDTIx | Under a heavy load of MWI traffic from IP to TDM, the PBX stops processing MWI requests from the Gateway when connected to a DMS100 PBX running ISDN NI-2 and cannot process simultaneous messages requests.
IPY00043959 | DMG100xLS | FSK data is not being completely recognized because TCID type 3 is not supported.
IPY00043910 | All | The Gateway experiences degradation in performance if the Gateway is requested to send many SIP messages over TCP to an IP endpoint (e.g. VoIP endpoint) that does not exist.
IPY00043919 | DMG2xxxDTIx | The Gateway gets into a state where it will continually retry failed VoIP-to-TDM routes if the initial route fails due to a Redirect request from the TDM network.
IPY00043918 | DMG2xxxDTIx | VoIP-to-TDM calls fail if the TDM network sends the Gateway a Redirect and the VoIP Host Address in the Routing Table is not '*'.
IPY00043992 | DMG100xLS | IP to TDM calls are connecting before the TDM call is actually answered.
IPY00044244 | DMG2xxxDTIx | "No Channels Available" alarm is generated when the consultation call is created on a different span than the original span because the first span has no channels available and there are channels available on a different span.
IPY00044360 | DMG2xxxDTIx | The Gateways generates a red alarm on ISDN during the midnight routine on a Nortel Meridian.
IPY00044694 | All | Browse buttons overlap a cell in the table on the Certificate page in Firefox.
IPY00044407 | All | Hidden outbound fields are not visible in Firefox.
IPY00044697 | All | On the router test page for VoIP Inbound, the VoIP endpoint and port cannot be entered.
IPY00044698 | All | In Firefox the Router and TDM test pages display “Requesting Data From Gateway”.
IPY00044411 | All | When VoIP Fault Tolerance is enabled the Gateway will not advance to the next host group. Busy or Not Available are reported and no connection to the next endpoint is attempted.
IPY00044449 | DMG2xxxDTIx | Boot sequence countdown is not displayed properly to the debug terminal.
IPY00044370 | DMG2xxxDTIx | T1 NI-2 A-LAW is not supported.
IPY00044371 | DMG2xxxDTIx | When an INVITE with Replaces is received the call handle is unknown.
IPY00044479 | All | Contact header is not present in SIP 202 REFER response.
IPY00044340 | DMG2060DTIx DMG2120DTIx | Alarm is generated when a transfer is successfully completed across spans.
IPY00074216 | DMG2xxxDTIx | Data abort exception is generated when redirecting name is manipulated through the routing table and a call is made from VoIP to TDM.
IPY00074213 | All | When a VoIP to TDM call receives a redirect request after the call information is manipulated through the routing table, the call log is incorrect for call manipulation on redirected TDM routing.

Release 6.0

May 9, 2008

Dialogic® Media Gateway models DMG2030DTI, DMG2060DTI, DMG2120DTI (T1/E1)

DMG2060DTIS, DMG2120DTIS (T1/E1 with Survivability) Requires:

File | Description | Version
t1e1_6.0.103.app | Gateway Application | |6.0.103|
T1E1_MR11.msd | DSP Firmware | |T1E1_MR11|
t1e1_6.0.103.fsh | Main CPU Boot | |6.0.103|
T1_LS_Cfg_Avaya8500.ini | Configuration file containing settings for Avaya 8500 T1-CAS Loop-Start | -
T1_LS_Cfg_Hicom300E.ini | Configuration file containing settings for Hicom 300E T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IMX.ini | Configuration file containing settings for NEC2400IMX T1-CAS Loop-Start | -
T1_LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC2400IPX T1-CAS Loop-Start | -
T1_LS_Cfg_LucentG3.ini | Configuration file containing settings for Lucent G3 T1-CAS Loop-Start | -

Dialogic® Media Gateway models DMG1004LS, DMG1008LS (Analog) Requires:

File | Description | Version
ls_6.0.103.app | Gateway Application | |6.0.103|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
ls_6.0.103.fsh | Main CPU Boot | |6.0.103|
LS_Cfg_Alcatel.ini | Configuration file containing settings for Alcatel PBX | -
LS_Cfg_Hicom300E.ini | Configuration file containing settings for HiCom 300 PBX (North America) | -
LS_Cfg_Hicom300ECS.ini | Configuration file containing settings for HiCom 300 PBX(Europe) | -
LS_Cfg_Mitel.ini | Configuration file containing settings for Mitel PBX | -
LS_Cfg_LucentDefinity.ini | Configuration file containing settings for Lucent Definity PBX | -
LS_Cfg_ATTSys25.ini | Configuration file containing settings for ATT System 25 PBX | -
LS_Cfg_NEC2400IPX.ini | Configuration file containing settings for NEC 2400 IPX PBX | -

Dialogic® Media Gateway models DMG1008MTLDNI (Mitel) Requires:

File | Description | Version
mtl_6.0.103.app | Gateway Application | |6.0.103|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.103.fsh | Main CPU Boot | |6.0.103|
MTLDNI_Cfg_Mitel.ini | Tone Definition config file for Mitel PBX | -

Dialogic® Media Gateway models DMG1008RLMDNI (Rolm) Requires:

File | Description | Version
mtl_6.0.103.app | Gateway Application | |6.0.103|
rrun_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
mtl46.lca | Telephony Interface Firmware | 4.6
mtl_6.0.103.fsh | Main CPU Boot | |6.0.103|
RLMDNI_Cfg_Rolm.ini | Tone Definition config file for ROLM PBX | -

Dialogic® Media Gateway models DMG1008DNI (DNI) Requires:

File | Description | Version
ami_6.0.103.app | Gateway Application | |6.0.103|
run_910FskEcho.dsp | DSP Firmware | |9.1 w/Fax|
inim653.iap | Telephony Interface Application | 6.53
iNim190.ilc | Telephony Interface Firmware | Platform 3 Build 190
iNim60.ibt | Telephony Interface Boot | 6.0
ami_6.0.103.fsh | Main CPU Boot | |6.0.103|
DNI_Cfg_Generic.ini | Tone Definition config file (generic) | -
DNI_Cfg_Hicom300E.ini | Tone Definition config file (DNI Hicom Optiset 300E 'European') | -
DNI_Cfg_Lucent.ini | Configuration file containing Adept rules for Avaya 7434ND and 8434 phones | -

Added Features:

FR # | Dialogic® Media Gateway Model | Description
FR2633 | All | The Gateway has been updated to support TDM-to-IP MWIs. Specifically, the DMG1000/DMG2000 will notify the specified VoIP endpoint when the gateway receives an indication from the TDM network that the VoIP endpoints message waiting indicator has been updated (set or cleared).
FR2838 | All | The Gateway has been updated to support the VoIP Failover and Load Balancing within the Dial Plan. This allows users to create Failover/Load Balancing rules on a per route basis.
FR2911 | DMG2xxxDTIx | The Gateway has been updated to allow users to configure the "Telephony Port Interface Side" parameter (Network Side or Terminal Side) on a per span basis for all T1/E1 ISDN protocols.
FR3013 | DMG2xxxDTIx | The Gateway has been updated to support the ISDN Divert message and reroute the VoIP-to-TDM call to the TDM destination identified by the Divert message.
FR3082 | All | The Gateway has been updated to include support for the 'ext' attribute on VoIP-to-TDM calls. Specifically, When the Gateway receives a 'ext' attribute as part of a VoIP-to-TDM call, the number contained in the 'ext' field becomes the number to dial.

Bug Fixes:

Defect # | Dialogic® Media Gateway Model | Description
IPY00074224 |  |
IPY00043928 |  |
IPY00074218 |  |
IPY00074274 |  |
IPY00043345 | DMG2xxxDTI | The Gateway may prematurely disconnect a VoIP-to-TDM call if the network does not send a PROCEEDING or a SETUP_ACK in response to the Gateway sending a SETUP message.
IPY00042608 | All | The Gateway does not echo the entire Referred-By header received in the REFER message during a transfer in the resulting Re-INVITE it generates.
IPY00042341 | All | The Gateway may parse the timestamp header of a received SIP message incorrectly resulting in the Gateway returning a 400 "Bad Request" response.
IPY00042224 | All | If the Gateway receives a SIP 302 message from the VoIP endpoint with multiple targets included in the Contact header, the Gateway will not send an INVITE to the subsequent targets in the list if the first fails.
IPY00039679 | DMG2xxxDTI | The Gateway does not support diversion information or MWI requests when connected to a E1 QSIG interface an Alcatel PBX that is configured for the ECMA format as opposed to the ISO format.
IPY00042202 | DMG1008LS | The Gateway does provide the correct Call Party Information when using the Serial MCI link connected to a NEC PBX that is part of series of NEC switches connected using Fusion link.
IPY00042088 | DMG2xxxDTI | The Gateway does not pass the Redirecting Party when configured for the E1 ETSI protocol.
IPY00042607 | All | Over time, the Gateway may stop communicating over the SIP interface after the Gateway receives Re-INVITE requests that are subsequently cancelled.
IPY00042827 | DMG1008LS | The Gateway allows the user to configure the unit to use the ETSI FSK protocol for gathering Call Party Information even though this protocol is not supported.
IPY00043339 |  | Duplicate of IPY00043345.
IPY00042529 | DMG2xxxDTI | On IP-to-TDM calls to a TDM phone that is busy, the Gateway responds with a 503 "Service Unavailable" message instead of a 486 "Busy Here" message when configured for an ISDN protocol
IPY00038091 | All | The Gateway may not be able to reboot if serial data is received across the serial integration port while the Gateway is rebooting.
IPY00043898 | All | The Gateway does not fully support Early Media (CIR IPY00043203)
IPY00043899 | DMG2xxxDTI | The Gateway fails a Consult Transfer if there are no free channels on the span that the original call is on even if there are free channels on other spans connected to the Gateway (CIR IPY00043008)
IPY00043900 | All | The Gateway may stop sending audio if it receives a Re-INVITE followed by an ACK where the SDP information is included in the ACK but not in the Re-INVITE (CIR IPY00043477)
IPY00043901 | All | The Gateway does not fully support Early Media (CIR IPY00042644)

Compatibility Notes:

Title | Description
Microsoft OCS - Voice Detection on ISDN | The Gateway may not send the SIP 200 OK response when the far end user answers the call until the user speaks on TDM-to-IP calls when using an ISDN protocol (e.g. QSIG, NI-2, etc.).
Microsoft OCS - Early Media | The Gateway is not compatible with the SIP Early Media feature as implemented on the Microsoft Mediation Server.
Norstar PBX DTMF | Norstar switches do not render DTMF digital station to digital station. This means that DTMF cannot be used to signal from a digital station to a DMG1000 port connected to a Norstar switch.
Avaya Legend PBX CPID | Avaya Legend switches do not provide redirecting call-party information when the call has been forwarded to a coverage-path to which the DMG1000 is a member. This means that DMG1000 will not be able to determine the called-party for inbound PBX calls that have been forwarded to a coverage-path.
Dial-Digit Relay Notes | There are 3 ways to achieve digit relay between the IP side and the TDM side. They are via the VoIP signal protocol, RFC2833 tones in RTP, or inband tones in RTP. For VoIp signal protocol, SIP does not yet support this. Drafts are in early stages. Therefore, we do not generate/receive signal digit relay on SIP (even though it is still part of the configuration). RTP digit relay, both inband-tone and RFC2833, works on SIP. Most SIP devices will render an actual tone when they receive an RFC2833 digit event, but they don't have to. The gateway will render an actual tone when it receives an RFC2833 digit event on SIP. Inband-tone works on both SIP and H.323, since it is actually going through the voice channel. But, some devices will remove the inband-tone from the voice stream.
Type II (Post-Answer) CPID | TDM-to-VoIP calls: when VoIP endpoint answers, first few seconds of audio may be clipped because audio is squelched during transmission of Type II CPID from the switch. On switch side of the call, the caller still receives ring-back tone while the switch is playing the Type II CPID tones.